Handbook on Optical Character Recognition and Document Image Analysis, pp. 000–000 Eds. H. Bunke and P. S. P. Wang

cfl 1996 World Scientific Publishing Company

CHAPTER 19

ANALYSIS OF PRINTED FORMS

DEBASHISH NIYOGI, SARGUR N. SRIHARI and VENU GOVINDARAJU CEDAR, SUNY at Buffalo, 520 Lee Entrance, Suite 202 Amherst, New York 14228-2567, USA

Automatic analysis of images of printed forms is a problem of both practical and theoretical interest, due to its importance in office automation, and due to the conceptual challenges posed for document image analysis. The automatic reading of optically scanned forms consists of two major components. The first is the extraction of the data image from the form; the second is the interpretation of the image as coded alphanumerics, and is commonly referred to as optical character recognition (OCR). The individual steps involved in forms analysis include image pre-processing, forms identification, field extraction, data interpretation, and contextual post-processing. In this chapter we outline the issues and current state-of-the-art in the analysis of printed forms. Forms analysis poses several challenges, given the enormous variety of current form layouts and contents, and some of these research issues are explored. In particular, two current forms analysis systems developed at CEDAR are described.

Keywords: Forms analysis; Forms editing; Data entry; Image pre-processing; Forms processing applications.

1. Introduction

A paper form is any preprinted document designed to elicit information. The problem of automatically interpreting an optically scanned and digitized image of a filled-out paper form containing typed and handwritten entries is considered in this chapter. The goal of forms analysis is to segment the form into the basic components of text (characters and words), line segments and boxes, and then analyze the components to extract relevant information from the form.

Forms analysis has grown to be a major component of document image understanding. Imaging-based technology, as well as several innovative forms analysis techniques, have made it much easier, quicker and cheaper to process the hundreds of different types of forms that typically need to be processed.

Most common documents that are processed are forms — even bank checks are nothing but small, simple forms. All kinds of organizations use forms: finance, education, retail, health care, shipping and transportation. Forms hasten market research, order entry, payment and delivery. Governments, especially, deal in a vast number of forms.

As industry and government interact with larger numbers of companies and people, the number of forms multiplies. Forms processing lets the user handle more data with the same number of people, and imaging to databases and data entry. 1

Instead of having many people keying in data off paper forms, forms processing extracts the data from images and uses it to populate databases.

In forms processing, one handles completed forms that arrive via fax or scanned documents. After cleanup and processing, the form images can be routed on a network or stored. After extracting the data from a form and verifying its accuracy, one does not need to keep the form. (One part, the signature, might need to be archived, but there is no need to record indefinitely whether someone filled in a box with a checkmark, an X, or a solid circle.) Once the correctly extracted data enters the database, the data becomes the important resource to safeguard and process, not the form from which it came.

1.1. Characteristics of forms

Forms are more complex and harder to work with than other imaging documents, due to the following [1]:

ffl They contain more than just text.

With documents, one can OCR the raw text (usually machine-readable, and created by typewriters, laser or dot matrix printers) and put it in a full-text database. One can also retrieve the images using index or keyword searches. Flexible text search engines allow the user to find text even if it contains many OCR errors. But forms can contain more than machine-readable text — they often come with checkmarks, handprint and signatures, all of which the system must recognize and process.

Even barcodes take on new weight with forms. While some systems use barcodes for auto-indexing images, form packages use them to identify the form or the provider of the form. Some users remove a peel-off barcode from an inventory item and stick it onto a form. The forms processing application converts the code to a number and uses it to modify the inventory database.

ffl They make data extraction more difficult.

Text-oriented OCR works with text in paragraph format. Such OCR systems do not typically look for text inside one-letter boxes, between lines, placed in different positions on the page, etc. Forms processing systems, on the other hand, need to OCR text in discrete chunks surrounded by graphic elements, such as lines and boxes and “combs”. Sometimes the text overlaps. Thus, OCR for forms packages have to recognize a character, even with lines dissecting it. With the line in place, the character is marred. With the line removed, the character is broken. Either way, recognition becomes difficult for OCR.

ffl They compress more slowly.

Forms contain lines, fancy type, logos and guide text (instructions that help users to fill the form). These elements hinder compression. Most compression algorithms, optimized for text and unbroken runs of white pixels, slow down when they have to process forms.The difference is similar to that between how fast one can fax a simple cover page and a busy page with a lot of text and graphics.

ffl They compress less efficiently.

Because it contains a lot of extra lines, fonts, logos and guide text, a compressed form can be four to 10 times the size of the same data without the form. Users can save space by dropping out the form and just compressing the data. A blank form can be stored at the user workstation and recombined with the data to display or print it. Doing this can boost performance and reduce storage needs by a factor of 10.

ffl They may contain data needed to process them.

In standard imaging systems, one can scan documents, index them, run them through OCR for full-text retrieval, then store them in one place. But with forms, one might perform different OCR operations on them to extract different types of data based on preliminary data that is read from the form (e.g., type of form).

ffl They involve handprint.

Forms are designed to be filled in by hand. However, handprinting is more difficult to read than machine-generated text, since there is more variation. Fortunately, forms present blocks or fields to constrain the handprint. Without these, standard OCR systems would have a difficult time reading a paragraph or a full page of handprint well. In forms analysis, context-based text reading becomes more important than simple OCR.

2. Background

Current research in forms analysis is ongoing at several universities and research institutions. Recent research papers in the area of forms processing describe various approaches towards the solution of different components of the overall forms processing problem.

Casey and Ferguson [2] describe a method developed at IBM for entry of a wide variety of forms that contain machine-printed data and that are often produced in business environments. The function, called Intelligent Forms Processing (IFP), accepts conventional forms that call for information to be printed in designated blank areas, but in which the information may exceed boundaries due to poor registration when printing. The IFP system uses a setup phase to create a model of each form that is to be read. Scanned forms containing data are compared against the matching form model. Special algorithms are employed to extract data fields while removing background printing (e.g., form lines) intersecting the data. The extracted data images are interpreted by an OCR process that reads typical monospace fonts. New fonts may be added easily in a separate design mode. If the data are alphabetic, a lexicon may be assembled to define the possible entries.

Taylor et al. [3] describe techniques for manipulating electronic images of forms in preparation of data interpretation. A combination feature extraction/modelbased approach is used for forms identification, registration, and field extraction. Forms identification is implemented with a neural network. The system is demonstrated on Internal Revenue Service forms.

Watanabe et al. [4] propose a new method to recognize the layout structure of table-form documents analytically. Their method identifies the line segments directly and interprets the layout structure with the extracted line segments. Traditional approaches to extract characters from table-form documents erase all line segments in order to utilize the character recognition techniques or apply the OCR techniques. In this approach, however, the mutual relationships among line segments is very important for the structure analysis because the line segments specify the document layout structure. In addition, the individual blocks partitioned by the line segments define the particular domains of meaningful items.

Yan et al. [5] propose a knowledge-based form understanding system for automatic data entry. It includes two parts, the design and implementation of a Form Description Language (FDL), and the understanding program. This system can process various kinds of forms and produce images of different items in the form in any desired order. Moreover, this system has learning capability. It can update the description according to its analysis so that it can understand the form more quickly and accurately afterwards.

Yuan et al. [6] introduce a new method for extracting the filled items from the pre-printed parts of a form by using an unfilled form as a model object, and a filled form as a moved version of the model. The motion is detected by a new technique called GRHT (generalized randomized Hough transform), and then the two forms are registered so that the filled items can be extracted by some simple operations.

Chandran and Kasturi [7] describe a system for the extraction of structural information of a table from its image. Following the initial binarization and deskewing operations, the image is analyzed to extract all horizontal and vertical lines that are present. The table’s dimensions are estimated based on these lines. Unlike other systems, this procedure does not depend on the sole existence of lines to mark the item blocks. White streams are recognized in both the horizontal and vertical directions as substitutes for any missing demarcation lines. A structure interpretation procedure uses the extracted demarcation information to identify each of the item blocks in the table. Subsequently, the inter-relations of these item blocks is used to recognize the structure of the tabulated data.

Monger et al. [8] describe the design and implementation of a user-friendly graphical package for the interactive layout and content description of document images. The specific problems addressed are those associated with predefined forms, such as proposal forms used in the insurance business, which have been completed by hand. The document image description allows position and content of the handwritten fields to be defined and labeled, and their inter-relationships specified. This information assists the automatic processing of handwritten forms using OCR techniques by enabling appropriate OCR algorithms and local syntax constraints to be applied to each field to produce the best recognition performance.

2.1. Forms Processing Research at CEDAR

Active research on forms processing has been ongoing at CEDAR (Center of Excellence for Document Analysis and Recognition). Research techniques developed at CEDAR have been implemented in current delivered products. The forms processing techniques developed at CEDAR that have been published so far include the following:

Wang and Srihari [9] describe an approach to the extraction of text, both typed and handwritten, from scanned and digitized images of filled-out forms. In decomposing a filled-out form into three basic components of boxes, line segments and the remainder (handwritten and typed characters, words, and logos), the method does not use a priori knowledge of form structure. Characters broken by line removal are rejoined using a character patching method.

Lam et al. [10] present a robust form reader with high adaptability and trainability. The form reader consists of two modules: field registration and data recognition modules. The field registration module acquires knowledge about the forms of interest, and the data recognition module recognizes text data on filled forms using the acquired knowledge. The capability of the reader increases progressively through supervised learning. The form reader has been trained to read a large variety of forms with machine-printed data. The adaptability and trainability of the system has been demonstrated through the experiments.

3. CEDAR Forms Analysis

Current research and development in forms analysis at CEDAR includes the use of forms processing techniques in several ongoing projects, including the Name and Address Block Reader project for reading IRS tax forms, and a Forms Analysis project for extracting information from business reply cards.

3.1. Name and Address Block Reader

In the Name and Address Block Reader (NABR) project, sponsored by IRS & Grumman Data Systems Corp., address block labels are extracted from IRS tax forms. Only the address block is received from the IRS tax forms, and data is extracted from these address blocks.

All but one of the forms have “drop-out” guidelines, which allow a person to fill out the form within the boundaries marked, but also allow the form to be processed electronically without the guidelines being present to interfere with the recognition of the characters. The only exception to the above is the IRS Form 1040EZ, which does not have drop-off guidelines. Therefore, for this form, the guidelines have to be first removed before any further processing.

Fig. 1 shows some examples of name-and-address blocks extracted from various IRS forms. The forms represented are:

(a) 1040EZ (non-dropout) (b) 1040EZ label

(c) 941 non-label (dropout) (d) IRPS non-label (dropout)

On receiving an image, this system first attempts to find out whether it is a label image or not. It is important to get the anchor points for proper registration of the 1040EZ non-label image owing to the non-dropout guide lines which interfere with the segmentation and recognition processes. A set of significant features such as shape and location of instructions found within the input image is used for the anchor information. Then the guide lines are removed, and the printed or handwritten information is extracted and sent to a segmentation process. The segmented image is further processed with a character recognition algorithm that identifies the individual characters in the label and then performs contextual postprocessing to correct any character recognition error.

It is not necessary to apply the anchor information for the non-label images in the other forms because of the use of dropout guide lines. Information of name, address, city, state and ZIP Code is extracted from the areas predefined according to the various forms.

For the label images in all forms, anchor information is also useful for proper process. Common anchor points are the Social Security Number with check digits or the identification numbers (Employer Identification Number, Payer’s Identification Number, or Recipient’s Identification Number). Extracted information is sent to a different character recognition algorithm designed for OCR-A font.

More details on this system can be found in [11].

3.2. Analysis of Reply Cards

The objective of this project is to develop a Forms Analysis system to analyze certain types of forms, e.g., postal reply cards. The system is designed to do the following:

(i) Acquire the images of the information-bearing side of the reply cards. (ii) Determine the recipient’s ID to determine the required service(s) and to retrieve relevant a priori information regarding that particular reply card.

(iii) Extract the information contents (both address and non-address) automatically.

(iv) Forward the image to a site for further manual processing, if automated processing fails.

(v) Organize the extracted information in a format specified by the recipient. (vi) Aggregate the processing results of the reply cards destined for the same recipient.

The system has the capability of processing both handwritten and machineprinted reply cards. Processing the reply cards involves reading both the address and non-address information. The speed of processing the addresses is 2.2 images per second for handwritten addresses and 2.8 images per second for machine-printed addresses. Fig. 2 shows the overall system functional design.

Fig. 1. Name and address blocks in IRS forms.

Fig. 2. Functional design of the CEDAR forms analysis system.

The demonstration system includes three different modules: (i) off-the-shelf forms processing product that can correct for skew, remove form guide lines, and extract sub-fields, (ii) OCR engine to read every sub-field in both the address and non-address sections of the reply card, and (iii) a reject re-entry software for manual processing of (some) reply cards.

A survey of forms processing software was performed as part of this project, and a forms processing package is part of the overall system. The forms processing software selected for this project needed to be reliable, require little end-user training, and be able to be interfaced in the overall design. Specifically, there were several tasks called for by the functional design. They were:

Form Definition — A user should be able to easily define zones to be extracted from a form through a comfortable graphical user interface.

Form Identification — The software should be able to identify a filled-in form reliably using a set of previously scanned blank forms.

Form Removal — The package should perform accurate form removal, even on low quality or skewed images.

Preprocessing — It is desirable, although not required, to have a package that performs some line and noise removal on the extracted zones.

Reject Re-entry — Images which cannot be accurately recognized by the system’s OCR should be displayed and highlighted to prompt the operator for corrective values if necessary.

The above tasks needed to be executed in real time as images are output from the scanner with the exception of the offline reject re-entry processing. This means that the forms processing software must be able to directly interface with the control structure written in C code.

3.2.1. Survey of commercial form readers

Most forms processing packages operate in a series of steps:

Zone Design — The user scans a blank form and defines all zones in which data to be recognized is contained. Zones are drawn with a mouse for easy and efficient definition. Attributes for all zones are compiled for use during recognition.

Scanning — Forms are scanned individually or in batches using a number of commercially available scanners suited to the application requirements. Variable data from the defined zones are stored for recognition.

Recognition — Images of the variable data are converted to ASCII and written to mass storage. All characters which cannot be accurately recognized are marked for post processing.

Post Processing — This paperless step may be performed when the user desires.

Each unrecognized character and all others within a zone are magnified and displayed in their original image form on the computer screen. The operator is then prompted to enter the correct character which is then placed in the output stream.

Data Transfer — Data is edited into the desired output format for transfer to other applications.

Several commercially available forms processing and OCR packages were included in the survey. They were: AEG, ComCom Systems Inc., Recognition Research Inc. (RRI), Recognition Inc., Nestor Inc., TiS America, Symbus Technology, and Sequoia Data Systems. Of these, the following products were evaluated in greater detail.

AEG 6160 ICR:

The AEG system is able to recognize characters at great speeds, but it is limited to machine-printed and upper-case-only hand-printed characters. It is currently not available for the Sun platforms and cannot be used for mail processing applications.

Nestor NestorReader ICR:

Nestor’s character recognition system is comprised of an all-software package. Hand and machine-printed alphanumeric character recognition is possible, with an advertised recognition rate of 99.8% on the NIST test set. Recognition can be done at a speed of 15 characters per second on a Sun SPARCstation. Segmentation of unconstrained touching characters can be done, and Nestor claims to handle sloppy writing and low resolution (Fax) degraded images.

TiS America FormOut!:

TiS America’s FormOut! contains only form identification and removal routines that can be interfaced with a C program. The software development kit programmer’s manual was used in detail to evaluate the system since it included examples of features available through the software. Noise, line, and skew removal is performed on the whole image during form removal, although the quality of these features appeared to be limited. Form definition was not very robust and required more effort than other packages.

RRI FIP2000:

RRI offers a complete forms processing package, from form identification, through form removal, and also reject re-entry. A demonstration copy of the system was obtained from RRI and helped greatly in the evaluation of the product. The task of defining a blank form is performed fairly easily by a user with little training. Attributes can be assigned to zones for use by the OCR downstream, and all image can be accessed through C functions. Reject re-entry provides two modes of operation. Individual character mode allows an operator to quickly process a continuous stream of rejected characters without regard to context. In full context mode, the rejected character is displayed with surrounding image data. RRI claims their research shows that allowing an operator to switch from one mode of work to the other actually increases overall productivity. Currently, the form definition and reject re-entry programs are not available for Sun SPARCstations, but are available for MS-DOS.

Based on the evaluation of the products mentioned above, RRI’s FIP2000 form removal package along with their reject re-entry program was found to best suit the needs of the Forms Analysis system. Feature qualities found to exceed those from other products include:

ffl Ease of blank form definition. Their FIPEdit program provided a comfortable graphical user interface for selecting zones for removal.

ffl Many C functions available in the FIP2000 library to allow all necessary data extraction required by the control structure.

ffl Fast forms processing. Processing time, including form identification and removal, was under 1 second for all test images.

ffl Moderate cost.

3.2.2. CEDAR forms processing software

The major tasks in the forms processing component of the system are Forms Registration, Forms Identification, and Forms Reconstruction. A forms editor is required to create the definition of each type of form that the system is required to process. A forms library is also necessary, so as to store the different form definitions.

RRI’s forms processing package has been replaced by a package developed at CEDAR. This task involved creating a forms editor, designing form definition files, and creating C library routines that can be linked by the programmer(s) of custom forms processing software. The library functions are used by the programmer(s) to write software for form identification, form removal and form reconstruction. The CEDAR forms processing package will serve this project as well as other forms processing projects.

The current status of the CEDAR forms processing software is as follows:

Forms Editor:

A forms editor must be easy for the user to use, yet be complex enough to handle the many different forms that it may come across. The CEDAR forms editor has a user friendly X Windows-Motif interface. There are menus and tool bar buttons that give the user access to editor features.

Menu options and pop-up windows enable users to specify control definitions and various user preferences. The user is able to create zones, fields, tags, lines and registration components to be saved to the form definition file. This form can be re-read by the editor for further definition or for visual feedback to the user. Processes allow the user to scroll on the image, zoom on the image and rotate the image. The user is also able to select form definition components. Once the form definition component is selected it can then be resized, moved or deleted. Also the editor allows the user to set attributes for fields and checkboxes. The editor has been integrated with the library so that form definitions produced with the editor are used by the library as input to the form processing.

Forms Library:

The forms library provides the user with a collection of functions that are important to forms processing. These library functions act on the images created by the forms editor. The high level processes are Forms Identification, Forms Removal and Reconstruction. A full specification has been developed for these functions.

Low level design work has provided a set of low level (internal) functions to be used by the Forms Processing Library. This helps keep the library relatively small. A high level specification finalizes the presentation of the library to the user. All main features of the library (with the exception for reconstruction) were integrated and tested to see a form through from registration to field snippets. This includes the library loading form definitions into memory. The library has been wrapped into high level user-callable functions according to the specifications.

Alternate forms of registration have been added to handle images that do not correspond to the final Reply Card specification. The library has undergone extensive testing with different combinations of user-available library functions being called. This quality assurance process ensures that the library (along with the editor) are in a state to be released.

3.3. CEDAR Data Entry

CEDAR has developed a field re-entry package on the Sun Sparc platform. We have used the experience gained here along with ideas learned from our analysis of several commercial data entry packages to develop a quality data entry system precisely suited for this application.

3.3.1. Data entry software

Recently a survey of data entry software was conducted as part of the ongoing Forms Analysis project. This survey compared the reject re-entry and manual entry features of various commercial forms processing packages, as well as the associated costs. Table 1 shows the comparison of the data entry features for these packages.

3.3.2. Design considerations

As mentioned above, CEDAR has surveyed over 20 forms processing and data entry companies in its endeavor to identify a commercial package that would fit the needs of the Forms Analysis project, and be easy to install and integrate with the rest of the system. We found that although several companies offer powerful data entry application development functionality, they require considerable effort to design applications. Some packages offered only simple re-entry of characters within a snippet field image, while most could not support importing of recognition data into their proprietary file format. Furthermore, none could directly make use of information stored in the form definition files.

After reviewing these packages, features were identified that would be attractive to users:

ffl A comfortable development environment which is simple to learn and use. ffl MS windows based.

ffl Quick application creation. ffl Drag and drop control of fields. ffl Provide many validations for field data.

ffl All options and controls available through pop-up windows. ffl Allow flexible image and data entry window placement. ffl Use of standard input and output file formats. ffl Allow entry of data for a whole image.

ffl Allow entry of data for selected snippet of the whole image. ffl Allow re-entry of recognition results with highlighting option of low confidence characters.

ffl Allow linking of fields to each other. ffl Tracking of operator keystroke statistics.

Analysis of Printed Forms 13

Table 1. Data entry software review

Company Reject Manual Notes Re-entry Entry

Autodata X Focus is auto data entry. Cardiff X Re-entry of their OCR’d data. ComCom X Re-entry of their OCR’d data. Computer Systems Co. No data entry.

DataCap X X Manual data entry possible with programming language provided. Applications cannot be easily created.

DataLex X Full feature Windows data entry, easy to integrate, no reject re-entry currently.

Diamond Head Powerful auto data entry system using Visual BASIC interface. Focus on image scanning and display. No data entry.

GTESS X Auto data entry and validation. Imagination No data entry. Kofax X X Recommended TextWare. Ligature X OCR’d text pages. Simple re-entry of page data. Maxsoft No data entry. Microsystems Tech. No response from company. Mitek X Re-entry of their OCR’d data. Principia X Mainly mark sense recognition with re-entry. Recognition International

X X They just redistribute TextWare’s DOS software. More powerful systems available.

RRI X Comfortable character re-entry tool. No snippet re-entry.

SCS X X OS/2 full featured image data entry. Difficult programmer interface. They suggest SCS setup for clients.

Solution Technology

No data entry, only image viewing.

SPSS X X Auto data entry with re-entry. No image based manual entry.

Tangent Systems No data entry.

TextWare X X Simple DOS based image data entry. Validation checks to handle most situations. Not very flexible.

TiS America No data entry, only forms processing. TurboPower Software

Borland C++ functions to do simple image data entry and validation.

3.3.3. Full data entry from images

No single commercially available data entry software package has all of the features needed by the Forms Analysis system. The CEDAR data entry package incorporates the desirable functionality described above and also introduces features that specifically benefit the system. These missing features include:

ffl Providing data entry and reject re-entry under one development environment in MS Windows.

ffl Use of form definition file attributes and image coordinates for data entry application design.

ffl Marking poor quality images for re-get and retrieval requests.

The data entry application development process is shown in Fig. 3. Users can create the forms definition manually using the specification of a reply card, or automatically using a form definition file for the card as defaults for field set up. The Screen Definition interface creates a definition file that is loaded into the Data Entry Processor interface along with a batch file describing which cards are to be processed (see Fig. 4). Several operators can be running Data Entry Processors on separate PCs to perform data entry in parallel.

Fig. 3. Screen definition process.

Fig. 4. Data entry process.

3.3.4. Screen definition

As mentioned previously, the data entry package provides a means to create data entry screens in one of two ways. The easiest way for screen development is to let the system create the screen definition based on attributes and image coordinates found in a corresponding form definition file. Using a form definition file, many of the field validations can be initialized. The screen developer only has to verify that these validation attributes are correct and enter any additional attributes that may be needed for data entry, but are not needed for recognition. Using form definition files to initialize the screen definition will leave the field order as it appeared in the form definition. After a screen has been defined using a form definition, the developer will have the ability to modify the screen definition in any manner to customize the screen for data entry.

If a form definition file is not to be used to initialize a screen definition, the data entry package gives the developer the ability to define all parts of the data entry screen. A screen window is drawn with the mouse by the developer to store a data entry window and image data. The data entry window holds the fields that the operator uses to enter the card data. The data entry window size and placement can be defined by drawing it with the mouse and it can be moved to any location within the screen window. Within the data entry window, fields are defined by dropping them with the mouse in the window. Default values are assigned to the field attributes initially, but can be changed through a popup attribute window.

The attributes available for a field include, but are not limited to:

ffl field name ffl title string ffl data display length data type ffl print type ffl classes ffl entry order number ffl output field number ffl image number ffl field image location (top, left, bottom, right) ffl check digit algorithm ffl double key flag ffl lexicon ffl range ffl required field ffl field mask ffl number of characters ffl case ffl default value ffl confidence threshold (for character highlighting) ffl highlight color ffl equation (to combine values from other fields) ffl checkbox group (to link checkboxes together)

The data entry order defaults to the order in which the fields were created, but this order can be changed. The screen developer can link snippet field images or their location within a full image to a data entry field. This information is stored in the associated field attributes.

3.3.5. Data entry processor

As shown in Fig. 4, operators run the Data Entry Processor interface to perform the actual manual data entry functions. The Data Entry Processor reads a batch file which specifies the reply card files that are to be processed and the screen definition file that should be used for the data entry interface. The Data Entry Processor screen is initialized using the screen definition file, and all attributes for each field would be applied as the operator goes from field to field. The Data Entry Processor executes in an efficient manner such that the operator will not be significantly impacted by the program’s processing overhead.

Operator keying statistics are output for each batch session. These statistics include items of interest common to typical data entry environments.

3.3.6. Data entry file interface

The Data Entry Processor is able to read standard TIFF format files as input. It is able to use full, removed, and snippet image data, along with field and character image coordinates. Recognition data is used to highlight low confidence characters for snippet verification and reject re-entry.

The Data Entry Processor writes the entered data to the Manual Results section of the input TIFF file. This data can then be converted to a format that is able to be imported to the clients database using standard utilities available through the current system.

3.3.7. Reject re-entry

In addition to the full data entry of reply card images and snippets, a reject re-entry program has been developed which allows an operator to verify or correct recognition results at the character level. The user is able to use this program integrated with the data entry program, or separately as a stand alone program. As shown in Fig. 5, the Character Re-entry Processor operates on form images specified in an input batch file and, given a confidence threshold, displays those character images that have recognition confidence values below the threshold.

The character images are displayed in a manner that allows efficient re-entry. Many character images are displayed on the screen at one time to provide the operator with a look-ahead buffer. If the value cannot be determined from the character image, the snippet field is displayed as a contextual aid.

If the operator believes that the form image is of poor quality, options are available through the reject re-entry interface allowing the operator to make the appropriate requests to the system. Keying statistics are tracked as in the data entry interface.

Fig. 5. Reject re-entry process.

3.3.8. Reject re-entry file interface

The Character Re-entry Processor is able to read standard TIFF format files as input. It uses the character coordinates and image data from snippet data in the TIFF file to display the individual characters, and the recognition result confidence values are used to determine which characters are to be displayed.

The Character Re-entry Processor combines the entered data with the already recognized data and writes this to the Manual Results section of the input TIFF file. This data can then be converted to a format that is able to be imported to the clients database using standard utilities available through the current system.

3.3.9. Commercial data entry package

In order to provide data entry and reject re-entry capabilities in the system in the short term, CEDAR has chosen two commercial packages based on our review of packages mentioned previously. This software closely satisfies the requirements of the system.

CEDAR has created interface routines that allow the commercial packages to “plug into” the Forms Analysis platform with little or no changes to existing software. This involves converting the TIFF files containing images and recognition data into a format that is readable by the commercial software. Additionally, interface routines have been written to convert the commercial packages’ output file format back to the TIFF format.

One key benefit of the CEDAR data entry software is its ability to read form definition files directly when creating data entry screens. All commercial packages create their own format data entry screen configuration files through a manual interface, allowing different validation checks to be specified for fields. CEDAR is investigating converting the form definition files to the commercial proprietary formats to be used in creating data entry interfaces.

4. Conclusions

We have given an overview of different concepts involved in the automatic analysis of printed forms. We have described the problem of forms analysis as the task of extracting accurate information using some knowledge of the structure of the form. Two systems developed at CEDAR, namely, the Name & Address Block

Recognition system and the CEDAR Forms Analysis system, have been described. In particular, the data entry subsystem of the latter has been described in detail. The capabilities of some commercial forms processing packages have also been highlighted. Forms analysis is one of the most active research areas in the field of document analysis, and much of the future research progress is expected to quickly lead to viable commercial products.

Acknowledgements

We are grateful to David Bartnik for providing much of the information on the CEDAR Forms Analysis system, including the data entry software comparison table. Thanks are also due to Dr. Yong-Chul Shin and Vemulapati Ramanaprasad, who provided details on the NABR project, and to Sridhar Parthasarathy for information on the CEDAR Forms Processing package.

References

[1] Lee Mantelman, Up to 98% labor savings with automated forms processing, Imaging Mag. 3, 9 (1994) 14–30.

[2] R.G. Casey and D.R. Ferguson, Intelligent forms processing, IBM Syst. J. 29, 3 (1990) 435–450.

[3] S.L. Taylor, R. Fritzson, and J.A. Pastor, Extraction of data from preprinted forms, Machine Vision and Appl. 5 (1992) 211–222.

[4] T. Watanabe, H. Naruse, Q. Luo, and N. Sugie, Structure analysis of table-form documents on the basis of the recognition of vertical and horizontal line segments, in Proc. ICDAR-91, 1991, 638–646.

[5] C.D. Yan, Y.Y. Tang, and C.Y. Suen, Form understanding system based on form description language, in Proc. ICDAR-91, 1991, 283–293.

[6] J. Yuan, L. Xu, and C.Y. Suen, Form items extraction by model matching, in Proc.

ICDAR-91, 1991, 210–218.

[7] S. Chandran and R. Kasturi, Structural recognition of tabulated data, in Proc. ICDAR- 93, 1993, 516–519.

[8] D. Monger, S. Leedham, and A. Downton, An interactive document image description for OCR of handwritten forms, in Proc. ICDAR-93, 1993, 524–527.

[9] D. Wang and S.N. Srihari, Analysis of form images, in Proc. ICDAR-91, 1991, 181–191. [10] S. Lam, L. Javanbakht, and S.N. Srihari, Anatomy of a form reader, in Proc. ICDAR- 93, 1993, 506–509.

[11] S.N. Srihari, Y-C Shin, V. Ramanaprasad, and D-S Lee, Name and address block reader system for tax form processing, in Proc. ICDAR-95, 1995, 5–10.